**MYC Notice to Competitors #5**

**Offshore Series (Shell Harbour Race)**

**Amendment to the SI**

**Delete**

9. The Finish
9.1 For the Shellharbour race, boats will finish by crossing a line bearing 090 degrees true from the northern breakwater at the entrance to Shellharbour Marina. Boats will record their finish times and promptly report to the Race Officer

**Insert**

6. The Start

ADD
6.3 If the RO deems that there is insufficient wind at the start time then the fleet will proceed to motor south until such time the skipper of Enigma deems the race will start. Racing will commence from that position.

9. The Finish
9.1 For the Shellharbour race, boats will finish by crossing a line bearing 230 degrees magnetic (from the yacht) to the northern breakwater at the entrance to Shellharbour Marina. Boats will record their finish times and promptly report to the Race Officer